Performance Evaluation of RIP, OSPF & EIGRP via Tunneling IPV4 to IPV6
Raza Zaman , Johri Abdullah, Farhan Nisar, Samad Baseer
Electronic Devices, Vol. 5, No. 2, 2016.
DOI: 
Link: 
Abstract:
Random nodes movement in GNS3 shows degradation in the network performance due to communication
between IPV4 to IPV6. The communication process from one node to another node consumes time that related to control
packets. In static networks, the chances of failure networks are due to bad configuration. However, in GNS3, the main reason
for the topology change is caused by the nodes movement with different kinds of protocols and shares their information
respectively.