Improving the Performance of the Power Monitoring Channel in Tehran Research Reactor (TRR)
Mohsen Ahmadnia
Electronic Devices, Vol. 6, No. 2, 2017.
DOI: 
Link: http://www.dline.info/ed/fulltext/v6n2/edv6n2_1.pdf
Abstract:
In this work, the fission chamber detector with 5 MW of power was tested in different locations of Tehran
Research Reactor pool. If the detector was located at the distance of 1 meter from the eastern edge of the reactor and at the
height of about 1.4 meters from the floor, it was the best location for detector counting but due to the different placements and
displacements in western part of the reactor, it was not possible unfortunately. The dead time for 3 MW of power had been
1.67% which was the best result in comparison with Monte Carlo Code.