Auto-calibration Frequency and the Coarse Error Elimination
Dragan Denic, Goran Miljkovic, Jelena Lukic, Miodrag Arsic and Milan Simic
Information Security Education Journal, Vol. 10, No. 2, 2023.
DOI: https://doi.org/10.6025/isej/2023/10/2/38-44
Link: https://www.dline.info/isej/fulltext/v10n2/isejv10n2_2.pdf
Abstract:
WHAT IS THE PROPOSAL FOR THE POSITION METERING TECHNIQUE? The position measurement method is
performed with a hybrid pseudo encoder deactivated by combining the pseudo encoder with the incremental code track. The combination of the two code tracks improves the measurement resolution. The proposed hybrid pseudo encoder includes the detector for the pseudo-code reading errors. This helps to decrease the autocalibration frequency and eliminates the coarse error. TECHNIQUE TESTING OF THE PROPOSED ENCODER ELECTRONIC BLOCK IN THE PRESENTED CODER AND CODER TRACK CONDITION.