Impact of Node Mobility on MANET Routing Protocols Models
Bhavyesh Divecha, Ajith Abraham, Crina Grosan, Sugata Sanyal
Journal of Digital Information Management, Vol. 5, No. 1, 2007.
DOI: 
Link: http://www.dirf.org/jdim/v5n1a4.asp
Abstract:
A Mobile Ad-Hoc Network (MANET) is a selfconfiguring network of mobile nodes connected by wireless links to form an arbitrary topology without the use of existing infrastructure. In this paper, we have studied the effects of various mobility models on the performance of two routing protocols Dynamic Source Routing (DSRReactive Protocol) and Destination-Sequenced Distance- Vector (DSDV-Proactive Protocol). For experiment purposes, we have considered four mobility scenarios: Random Waypoint, Group Mobility, Freeway and Manhattan models. These four Mobility Models are selected to represent possibility of practical application in future. Performance comparison has also been conducted across varying node densities and number of hops. Experiment results illustrate that performance of the routing protocol varies across different mobility models, node densities and length of data paths.