Analytical Magnitude Optimum Criterion using the Rotor Field Oriented (RFO) Control Algorithm
Bojan Bankovic, Milutin Petronijevic, Nebojsa Mitrovic, Vojkan Kostic, Filip Filipovic
Journal of E - Technology, Vol. 12, No. 3, 2021.
DOI: https://doi.org/10.6025/jet/2021/12/3/67-75
Link: https://www.dline.info/jet/fulltext/v12n3/jetv12n3_1.pdf
Abstract:
For electric drives, the PI controller is the core component part of the control algorithm. It results in a better wide range application and represent the important part of the engineering learning. Integrated Education Platform for controllers tuning using graphic user interface in dSPACE ControlDesk environment. Analytical Magnitude Optimum Criterion is used for controllers tuning in the case of the Rotor Field Oriented (RFO) control algorithm. For testing we have implemented the dSPACE DS 1103 control board and tested in the laboratory for performance.