Fast and Accurate Practical Positioning Method using Enhanced-Lateration Technique and Adaptive Propagation Model in GSM Mode : Case Study Using Android Smart Phone in Egypt Roads
Mohamed Abdel Meniem1, Eman Shaaban, Ahmed Hamad
Progress in Signals and Telecommunication Engineering, Vol. 3, No. 1, 2014.
DOI: 
Link: http://www.dline.info/pste/fulltext/v3n1/1.pdf
Abstract:
In this paper, we consider problem of positioning of mobile phones, different approaches were produced for these targets using GPS, WiFi, GSM, UMTS and other sensors, which exist in today smart phone sensors. Location awareness in general is emerging a tremendous interest in different fields and scopes. Position is the key element of context awareness. However GPS produces an accurate position, it requires open sky and does not work indoors. We produce an innovative robust technique for positioning which could be applied on terminal-based or network-based architecture. It depends only on Received Signal Strength (RSS) and location of Base Transceiver Station (BTS). This work has been completely tested and analyzed in Egypt roads using realistic data and commercial android smart phone. In general, all performance evaluation results were good. Mean positioning error was about 120 m in urban and 394 m in rural.