Directional and Omnidirectional Antenna for Ricean and Rayleigh Channels
Oleg Borisov Panagiev
Progress in Signals and Telecommunication Engineering, Vol. 10, No. 1, 2021.
DOI: 
Link: https://www.dline.info/pste/fulltext/v10n1/pstev10n1_2.pdf
Abstract:
The Tx and Rx antennas are used for Television broadcasting and the differences between them are documented in this work. We have studied the directional and omnidirectional antenna for Ricean and Rayleigh channels. With the help of graphical presentations we have compared them with the ETSI requirements and further we did experimental observations.