Performance Evaluation of an Efficient Schduling Algorithm for Surviellance Monitoring System Using WiMAX
Noaman Abduljabbar Ramadhan, Rahiman A.R, Abdullah M, Zuriati A.Z
Electronic Devices, Vol. 7, No. 1, 2018.
DOI: 
Link: 
Abstract:
The application areas of video surveillance are increased in recent days. It is mostly used in static areas such
as airport, train stations, shopping malls and road traffic signals. In particular WIMAX networks were expected to support
several broadband technologies that provide various services which are video surveillance, audio and data. These services
include different classes of Quality of Service (QoS). Scheduling in WiMAX is one of the most challenging issues since it might
distribute its resources to all the users in the network. So, an effective scheduling is very critical in WIMAX networks. More
number of scheduling algorithms is available for WiMAX network. In this paper we propose a Priority Queue (PQ), Time
expire (TE) scheduling and hybrid between (TE and PQ) queue scheduling algorithms. In this paper we take video, audio
and text data for analyzing which one can efficiently support these three scheduling algorithms between (TE and PQ) queue
scheduling.