Measuring the Outage Probability of the System Over the Shadowed Rician Fading Satellite-relay Link and Rayleigh Fading Relay-user Channels
Aleksandra M. Cvetkovic, Jelena A. Anastasov and Nemanja M. Zdravkovic
Journal of Data Processing, Vol. 12, No. 1, 2022.
DOI: https://doi.org/10.6025/jdp/2022/12/1/16-24
Link: https://www.dline.info/jdp/fulltext/v12n1/jdpv12n1_3.pdf
Abstract:
In this paper, we have tested the outage performance of satellite terrestrial multiuser network using the fixed gain ample relays. We have arrived at the new derivation of cumulative distribution function of the highest end-to-end signalto- noise ratio (SNR) with the help of the opportunistic scheduling strategy. We have experimented the outage probability of the system over the shadowed Rician fading satellite-relay link and Rayleigh fading relay-user channels. Using simulations, we have measured the compact numerical results and analysed the impact of the number of service users and also the effect of mean SNR values.