Analysis of Probe-coupled Cylindrical Microwave Cavity with Plan Parallel and Dielectric Layers
Tijana Dimitrijevic, Jugoslav Jokovic and Bratislav Milovanovic
Journal of Electronic Systems, Vol. 13, No. 3, 2023.
DOI: https://doi.org/10.6025/jes/2023/13/3/75-83
Link: https://www.dline.info/jes/fulltext/v13n3/jesv13n3_3.pdf
Abstract:
The probe-coupled cylindrical microwave cavity with plan parallel and dielectric layers is analyzed. We discuss testing a compact wire model used in the 3D TLM cylindrical mesh for analysing the dielectric layers. The wire structures parameter measures help the implementation of the compact wire model. The conditions include the cross-section variables of the TLM nodes where the wire conductor passes in the cylindrical grid with a wire path. Implementing the compact wire model into a cylindrical TLM mesh is based on the calculation of wire structure parameters. The results are obtained and compared with plan parallel dielectric permittivity studies. For testing the TLM-based approach for characterization of a cylindrical metallic cavity loaded.