CDMA Time-hopping Optical Network with Enhanced Security
A. A. Ortega, V. A. Bettachini, J. I. Alvarez-Hamelin
Journal of E-Technology, Vol. 3, No. 4, 2012.
DOI: 
Link: http://www.dline.info/jet/fulltext/v3n4/3.pdf
Abstract:
A method to provide cryptographically secure point-to-point and point-to-multipoint communication using an encrypted Bloom filter is implemented on a time-hopping CDMA optical fiber network. A novel Hammingweight minimization coding algorithm optimises the performance of the encrypted Bloom filter in terms of end-user bandwidth utilisation over previous proposals. The system has a total channel utilisation of up to 29% for 128 simultaneous users, up to 20 km apart, served by a single passive optical hub, or longer distances if served by an active hub.