Clutter Mitigation of MTI Radar by Moderation of Blind Speed
Muhammd Saleem, Abdullah Sadiq, M.R. Anjum
Journal of Information Organization, Vol. 6, No. 2, 2016.
DOI: 
Link: 
Abstract:
 In radar system to achieve high visibility of clutter, blind speed personate severe limitation on the proper detection and tracking of MTI radar. By changing the pulse repetition interval which can increase the tolerable values of the blind speed. A severe problem may arise in the form of blind Doppler, no detection of target. To eliminate these blind speeds possible method of PRF staggering is used. Instead of using two radar to alleviate the blind speed of two different PRF,s single radar can minimize the effect of blind speed by two or different PRFs. in this paper systematic method is designed to eliminate the blind speed.