A New Method for Polarization Improvement
Yordan Kechev, Peter Petkov and Mario Gachev
Journal of Information Organization, Vol. 12, No. 2, 2022.
DOI: https://doi.org/10.6025/jio/2022/12/2/43-50
Link: https://www.dline.info/jio/fulltext/v12n2/jiov12n2_3.pdf
Abstract:
For the pin-fed patch antennas, we have developed a new method for polarization improvement. To ensure two orthogonal pin excitation, the stacked patch is deployed. To ensure more bandwidth and dual polarization, we have used the two orthogonal pin excitations. To confirm the low cost and compatibility with standard PCB manufacturing process we have used the RO4003 substrates. Finally, we have performed testing with full wave 3D FEM simulator HFSS.