Enabling More Energy Capacity of the Metal Oxide Surge Arrestors
Margreta Vasileva and Marinela Yordanova
Journal of Information & Systems Management , Vol. 13, No. 1, 2023.
DOI: https://doi.org/10.6025/jism/2023/13/1/1-9
Link: https://www.dline.info/jism/fulltext/v13n1/jismv13n1_1.pdf
Abstract:
The reasons for lightning strokes in circuits are mainly due to the overloading of metal-oxide surge arrestors. This process leads to the resistors-breakdown in surface discharges. Thus, the requirement in this stage to ensure more energy capacity which should be more than the energy loading. We in this work studied the protective operation and energy capacity of the metal-oxide surge arrestors. The impact of different lighting strokes and thermal loading are considered in this work. The result of this study is the creation of new systems the more production of energy required.