A Digital Video Watermarking Algorithm Based on LSB and DCT
Kirti Jain, U.S.N Raju
Journal of Information Security Research, Vol. 6, No. 3, 2015.
DOI: 
Link: http://www.dline.info/jisr/fulltext/v6n3/v6n3_3.pdf
Abstract:
In this paper a new watermarking algorithm is proposed for videos. The developed method embeds a binary
image as watermark into a colour avi video..In the proposed method, LSB and DCT both are embedded in the video frames.
We compare our algorithm with 2-LSB using Peak signal-to-noise ratio (PSNR). Experimental results show that the quality
of the watermarked image is higher. PSNR value is 63.74db in proposed method. This is higher compare to the other method.