Performance Measure and Analysis of MPLS and conventional IP network through VoIP: Effect in Video and Audio transmission
Jawad Oubaha, Abderrahmane Ez-zahout
Journal of Networking Technology, Vol. 9, No. 2, 2018.
DOI: 
Link: http://www.dline.info/jnt/fulltext/v9n2/jntv9n2_3.pdf
Abstract:
For the mapping the network interconnection of the different technology MPLS backbone and the wireless
network WiFi, we have only one choice to ensure the Quality of service the end-to-end. It is the service mapping considering as
the future solution to ensuring the performance traffic engineering between Label Switch Path "LSP" of MPLS and access
Category "AC" of IEEE802.11e wireless. This paper will propose the mapping between these technologies with Fuzzy logic to
optimize the quality of service in MPLS networks. MPLS and 802.11e is very useful approach for todayâ€™s things, the internet of
Big Data to keep a level of the Quality of service the end-to-end. It studies about different approaches to map 802.11e Access
Categories (AC) to Label Switched Path (LSP) and their contributions. It then introduces the concept of encapsulated LSPs
with Fuzzy to achieve future QoS, which requires an in-depth study to examine its practicability.