Modeling and simulation of non-linear or hysteresis behavior of magneto-rheological dampers in the example of quarter-car model
Sulaymon Eshkabilov
Progress in Machines and Systems, Vol. 5, No. 2, 2016.
DOI: 
Link: 
Abstract:
This paper presents reviews of numerical simulation models of non-linear and hysteresis behaviors of magneto-rheological liquiddampers in MATLABÂ®/SimulinkÂ® in the example of quarter-car model of vehicle suspensionsimulation, such as, Bingham, Dahl, LuGre and Ben-Wouc models.In addition, it discusses numerical results from simulation models for four different input excitations from terrain in order to analyze system performances in terms of car body displacement.