Two-layer Grounding Grids Using Computational Procedures
Marinela Yordanova, Margreta Vasileva, Rositsa Dimitrova
Progress in Machines and Systems, Vol. 12, No. 1, 2023.
DOI: https://doi.org/10.6025/pms/2023/12/1/1-10
Link: https://www.dline.info/pms/fulltext/v12n1/pmsv12n1_1.pdf
Abstract:
In the work we have developed a system to record two-layer soil structure by calculating the mesh voltage Em. We have used the computational procedure of the standard IEEE 80-000. We have used the formula for homogeneous structure soil with horizontal stratified medium. We have also used a formulae of equivalent resistivity. We have arrived at the Em values based on regular shape of grounding grids.