Self-Tuning Low Noise Amplifier During One Design Pattern
Goran Jovanovic, Darko Mitic, Mile Stojcev and Tatjana Nikolic
Signals and Telecommunication Journal, Vol. 11, No. 2, 2022.
DOI: https://doi.org/10.6025/stj/2022/11/2/41-48
Link: https://www.dline.info/stj/fulltext/v11n2/stjv11n2_3.pdf
Abstract:
We have carried out the self-tuning low noise amplifier which is normally termed as One design pattern. To equal the input signal frequency, we developed the phase control loop where the aim is to force the filter central frequency by changing the amplifier resonant. The LNA parameter has consistent maximum gain with good frequency and ensure full tuning for parameter perturbations. We have used the design of BICOMOS technology for confirming the LNA. The experimentation shows the full noise is optimum during the use of compression points.