A Coarse-to-Fine Registration Method Based on Geometric Constraints of Block and Parallel Architecture
Zetao Jiang, Chuan Guo
Transactions on Machine Design, Vol. 4, No. 1, 2016.
DOI: 
Link: http://www.dline.info/tmd/fulltext/v4n1/tmdv4n1_2.pdf
Abstract:
Aiming at long registration time and mismatch problems resulted by images that exist local region similar or
generated SIFT vector similar in the traditional SIFT registration method, a fine registration method based on geometric
constraints of block and parallel architecture is put forward. This method using SIFT algorithm parallelly extract feature
points to calculate initial transform matrix, in order to provide geometric constraints for block and fine registration, after
segment the overlapping region into several blocks, we do blockwise SIFT matching using parallel architecture to achieve
fine registration. During the fine registration, we use affine invariance of Mahalanobis distance to screen feature points and
eliminate duplicate matches and mismatches. The experimental results show that this method eliminates the mismatch generated
by same local features, registration accuracy and speed has improved, the proposed approach has practical value.