Double Squirrel Cage of a Three-Phase Induction Motor
Blagoja Arapinoski, Mirka Popnikolova Radevska, Vesna Ceselkoska
Transactions on Machine Design, Vol. 10, No. 2, 2022.
DOI: 
Link: https://www.dline.info/tmd/fulltext/v10n2/tmdv10n2_1.pdf
Abstract:
In this paper we have used the double squirrel cage of a three-phase induction motor and created systems using architecture. We have used the finite elements of the 3D domains to calculate the three-dimensional magnetic fields. We have also developed parameters to do so. Further the equivalent inductance of the machine with the load currents and used angular position of the rotors. This process helped to measure the leakage in the machine parts and also the measurement of electromagnetic torque. We have arrived at the results during experimentation and presented them in this paper.