3D Motor Simulation using Low Pass Filters and Magnitude Response Measures
Veljko Crnadak, Sinisa Tasic
Transactions on Machine Design, Vol. 11, No. 2, 2023.
DOI: https://doi.org/10.6025/tmd/2023/11/2/43-52
Link: https://www.dline.info/tmd/fulltext/v11n2/tmdv11n2_2.pdf
Abstract:
Using the lumped elements, we have prepared the design of the Chebyshev low pass filter. When the filter with magnitude response is applied, a ladder network with inductor series for shunt capacitors is generated. Initially, we transformed the low pass filter with real lossy reactive elements and then simulated the 3D EM simulator. To experiment with the design created, we simulated the filter obtained the values for S-parameters and compared them. In a frequency value of < 200 MHz, the low pass filter is found to have minimal insertion loss. The filter aims to limit the harmonics during high amplifier output.